This Imaging Configuration is designed to be used with the following Ink & Media combination: 

-Ink: Epson UltraChrome DS, T741x00
-Media:	Epson DS Transfer Production transfer paper (S0455xx), Yarrington Mills MicroPoly/Lycra Performance BODY FLEX fabric
-Halftone: Precision Stochastic Screens

The printer must be configured in the following manner:
-Media Type Set to: Front Panel Settings
Under Media Setup, select Customize Settings, and select an available slot, press Ok. On each of the options, configure the media with the following settings:
Setting Name: DS Production
Feed Adjustment: It is recommended to do a feed adjustment after configuring the other settings.
Platen Gap: 1.5
Head alignment: It is recommended to do 'bi-directional' and 'dual head' head alignments after configuring the other settings.
Drying - Heater Temperature: off
Drying - Drying Time Per Pass: 0 seconds
Media Suction: 5
Head Movement: Printer Full Width
Multi-Strike Printing: Off
Roll Type: Printable Side Out
Tension Movement: Periodically
Media Tension: Manual, 19
Feed Speed: 2
Takeup Tension: Auto

The heat press must be configured in the following manner:
-Press Temperature: 392F
-Prepress Time: 45 seconds
-Press Time: 25 seconds
-Press Pressure: 70psi
-Lint Roller used before prepress
-Two sheets of craft paper beneath fabric