This Imaging Configuration is designed to be used with the following Ink & Media combination: 

-Ink: Epson UltraChrome DS, T741x00
-Media:	Epson DS Transfer - Multi-Purpose Transfer Paper, Universal Woods Unisub ChromaLuxe Glossy White
-Halftone: Error Diffusion

The printer must be configured in the following manner:
-Media Type Set to: Front Panel Settings
In the Media tab on the front panel, select Custom Paper Settings, then select an available media slot, and press Ok. On each of the options, configure the media with the following settings:
Setting Name: Epson DS MP
Feed Adjustment: It is recommended to do a feed adjustment after configuring the other settings.
Platen Gap: 1.5
Head alignment: It is recommended to do 'bi-directional' and 'dual head' head alignments after configuring the other settings.
Drying - Heater Temperature: off
Drying - Drying Time Per Pass: 0 seconds
Media Suction: 5
Head Movement: Printer Full Width
Multi-Strike Printing: Off
Roll Type: Printable Side Out
Tension Movement: Periodically
Media Tension: Manual, 19
Feed Speed: 2
Takeup Tension: Auto

The heat press must be configured in the following manner:
-Press Temperature: 400F
-Prepress Time: None
-Press Time: 75 seconds
-Press Pressure: 55psi
-Layering of items inside the heat press from bottom to top: Nomex pad, two sheets of craft paper, Unisub ChromaLuxe substrate, transfer paper, sheet of craft paper, scrap fabric on top of transfer paper and craft paper